SECTION 10550
(New SECTION 105513)

MAILBOXES

Display hidden notes to specifier. (Don't know how? Click Here)
PART  1	  GENERAL
1.1 		SECTION INCLUDES
A.		Brass Mailboxes.
1.		Front-loading interior mailboxes.
2.		Rear-loading interior mailboxes.
1.2 		RELATED SECTIONS
A.		Section 04800 - Masonry Assemblies.
B.		Section 05400 - Cold Formed Metal Framing: Framed wall openings to receive mailboxes.
C.		Section 06100 - Wood Framing: Framed wall openings to receive mailboxes.
D.		Section 09250 - Gypsum Board.
1.3 		REFERENCES
A.		Architectural and Transportation Barriers Compliance Board (ATBCB):  Americans with Disabilities Act Accessibility Guidelines (ADAAG) for Buildings and Facilities.
B.		IBC - International Building Code.
C.		ASTM A 666 - Specification for Austenitic Stainless Steel Sheet, Strip, Plate and Flat Bar.
D.		ASTM B 209 - Specification Aluminum and Aluminum Alloy Sheet and Plate.
E.		ASTM B 221 - Specification Aluminum and Aluminum Alloy Extruded Bar, Rods, Wire, Shapes, and Tubes.
1.4 		SUBMITTALS
A.		Submit under provisions of Section 01300.
B.		[ Product Data ]:  Manufacturer's data sheets on each product to be used, including:
1.		Construction details, material descriptions, dimensions and finishes.
2.		Preparation instructions and recommendations.
3.		Storage and handling requirements and recommendations.
4.		Installation methods.
C.		Shop Drawings:  Prepared specifically for this project; show dimensions of mailboxes, wall cuts, and interface with other products.
D.		Selection Samples:  For each finish product specified, two complete sets of color chips representing manufacturer's full range of available colors and patterns.
E.		Verification Samples:  For each finish product specified, two samples, minimum size 2 inches (50 mm) square, representing actual color and texture.
1.5 		REGULATORY REQUIREMENTS
A.		Comply with Americans with Disabilities Act Accessibility Guidelines (ADAAG).
1.6 		QUALITY ASSURANCE
A.	 	Manufacturer Qualifications:  Manufacturer shall have a Quality System in place to ensure and be able to substantiate that manufactured units conform to requirements and match the approved design and must be ISO 9001:2015 certified.
1.7 		DELIVERY, STORAGE AND HANDLING
A.		Inspect the materials upon delivery to ensure that specified products have been received.
B.		Store materials protected from exposure to harmful weather conditions.
C.		Handle materials to prevent damage or marring of finish.
1.8 		WARRANTY
A.		Manufacturer's standard warranty to repair or replace components of postal specialties that fail in materials or workmanship within one year from date of Substantial Completion.
PART  2	  PRODUCTS
2.1 		MANUFACTURERS
A.		Acceptable Manufacturer: Salsbury Industries, 18300 Central Avenue, Carson, CA 90746-4008; Toll Free Tel: 800-MAILBOX (800-624-5269); Fax: 800-624-5299; Email: salsbury@mailboxes.com; Web: www.mailboxes.com
B.		Substitutions:  Not permitted.
C.		Requests for substitutions will be considered in accordance with provisions of Section 01600.
2.2 		BRASS MAILBOXES
A.			Private Delivery Front-Loading Brass Mailboxes:  Mailboxes with die-cast brass doors as manufactured by Salsbury Industries consisting of multiple compartments enclosed within recessed wall box. Provide access to compartments for distributing incoming mail from the front of unit with accessibility to entire group of compartments. Provide access to each compartment for removing mail by swinging compartment door.
1.		Model:  2000FL Series.
a.		Model 2030FL: 30 Door Unit - 3.5 inches (89mm) wide by 5 inches (127mm) high doors.
b.		Model 2016FL : 16 Door Unit - 5.5 inches (127mm) wide by 6 inches (152mm) high doors.
c.		Model 2014FL: 14 Door Unit -  (12) 5.5 inches (127mm) wide by 6 inches (152mm) high doors and (2) 11 inches (279mm) wide by 6 inches (152mm) high doors
d.		Model 2008FL: 8 Door Unit - 11 inches (279mm) wide by 6 inch (152mm) high doors.
2.		Mounting:  Recessed mounted.
3.		Locks:
a.		Key Lock – Standard: 5-pin cylinder cam lock, 2 keys per lock.
b.		Combination Lock – Three digit single dial with spring latch and automatic throw-off (not available on #3 doors).
c.	 	Non-Locking Thumb Latch - Custom.
4.		Box Identification:
a.		Engraved Plastic Windows.
I.	Clear Window.
II.	Tan-colored Window.
b.		Self-adhesive Numbers.
c.		Label Holders.
5.		Mail Distribution:
a.		Mail Distribution: Private.
6.		Compartment Material and Finish:  20 gauge steel with powder coated finish.
a.			Color:  Tan - standard.
7.		Door Material and Finish:  Die-cast solid brass with ¼” thick glass window.
a.			Color:  Clear - standard.
8.		Accessories:
a.		Hinged Locking Rear Cover.
b.		Trim Kit.
c.		Key Blanks.
d.		Plastic Windows.
B.		Private Delivery Rear-Loading Brass Mailboxes:  Mailboxes with die-cast brass doors as manufactured by Salsbury Industries consisting of multiple compartments enclosed within recessed wall box. Provide access to compartments for distributing incoming mail from the rear of unit with accessibility to entire group of compartments. Provide access to each compartment for removing mail by swinging compartment door.
1.		Model:  2000RL Series.
a.		Model 2030RL: 30 Door Unit - 3.5 inches (89mm) wide by 5 inches (127mm) high doors.
b.		Model 2016RL : 16 Door Unit - 5.5 inches (127mm) wide by 6 inches (152mm) high doors.
c.		Model 2014RL: 14 Door Unit -  (12) 5.5 inches (127mm) wide by 6 inches (152mm) high doors and (2) 11 inches (279mm) wide by 6 inches (152mm) high doors
d.		Model 2008RL: 8 Door Unit - 11 inches (279mm) wide by 6 inch (152mm) high doors.
2.		Mounting:  Recessed mounted.
3.		Locks:
a.		Key Lock – Standard: 5-pin cylinder cam lock, 2 keys per lock.
b.		Combination Lock – Three digit single dial with spring latch and automatic throw-off (not available on #3 doors).
c.	 	Non-Locking Thumb Latch - Custom.
4.		Box Identification:
a.		Engraved Plastic Windows.
I.	Clear Window.
II.	Tan-colored Window.
b.		Self-adhesive Numbers.
c.		Label Holders.
5.		Mail Distribution:
a.		Mail Distribution: Private.
6.		Compartment Material and Finish:  20 gauge steel with powder coated finish.
a.			Color:  Tan - standard.
7.		Door Material and Finish:  Die-cast solid brass with ¼” thick glass window.
a.			Color:  Clear - standard.
8.		Accessories:
a.		Hinged Locking Rear Cover.
b.		Trim Kit.
c.		Key Blanks.
d.		Plastic Windows.

PART  3	  EXECUTION
3.1 		EXAMINATION
A.		Verify that openings in wall are correctly located, aligned, and sized for mailboxes.
3.2 		PREPARATION
A.		Clean surfaces thoroughly prior to installation.
3.3 		CLEANING
A.		Clean surfaces with mild dish detergent.  Do not use harsh abrasive cleaners.  Lubricate locks with graphite type lubricants only.
3.4 	INSTALLATION
A.		Install in accordance with manufacturer's instructions.
3.5 		PROTECTION OF INSTALLED PRODUCTS
A.	 	Protect finishes from damage by construction activities.
END OF SECTION