SECTION 10550
(New SECTION 105513, 105516, 105523, 105526)

MAILBOXES

Display hidden notes to specifier. (Don't know how? Click Here)
PART  1	  GENERAL
1.1 		SECTION INCLUDES
A.		Aluminum Mailboxes – Rack Ladder System:  Rear Loading.
1.2 		RELATED SECTIONS
A.		Section 04800 - Masonry Assemblies.
B.		Section 05400 - Cold Formed Metal Framing: Framed wall openings to receive mailboxes.
C.		Section 06100 - Wood Framing: Framed wall openings to receive mailboxes.
D.		Section 09250 - Gypsum Board.
1.3 		REFERENCES
A.		Architectural and Transportation Barriers Compliance Board (ATBCB):  Americans with Disabilities Act Accessibility Guidelines (ADAAG) for Buildings and Facilities.
B.		IBC - International Building Code.
C.		ASTM A 666 - Specification for Austenitic Stainless Steel Sheet, Strip, Plate and Flat Bar.
D.		ASTM B 209 - Specification Aluminum and Aluminum Alloy Sheet and Plate.
E.		ASTM B 221 - Specification Aluminum and Aluminum Alloy Extruded Bar, Rods, Wire, Shapes, and Tubes.
1.4 		SUBMITTALS
A.		Submit under provisions of Section 01300.
B.		[ Product Data ]:  Manufacturer's data sheets on each product to be used, including:
1.		Construction details, material descriptions, dimensions and finishes.
2.		Preparation instructions and recommendations.
3.		Storage and handling requirements and recommendations.
4.		Installation methods.
C.		Shop Drawings:  Prepared specifically for this project; show dimensions of mailboxes, wall cuts, and interface with other products.
1.5 		REGULATORY REQUIREMENTS
A.			Comply with USPS-STD for wall-mounted centralized mailboxes.
B.		Comply with Americans with Disabilities Act Accessibility Guidelines (ADAAG).
1.6 		QUALITY ASSURANCE
A.	 	Manufacturer Qualifications:  Manufacturer shall have a Quality System in place to ensure and be able to substantiate that manufactured units conform to requirements and match the approved design and must be ISO 9001:2015 certified.
1.7 		DELIVERY, STORAGE AND HANDLING
A.		Inspect the materials upon delivery to ensure that specified products have been received.
B.		Store materials protected from exposure to harmful weather conditions.
C.		Handle materials to prevent damage or marring of finish.
1.8 		WARRANTY
A.		Manufacturer's standard warranty to repair or replace components of postal specialties that fail in materials or workmanship within one year from date of Substantial Completion.
PART  2	  PRODUCTS
2.1 		MANUFACTURERS
A.		Acceptable Manufacturer: Salsbury Industries, 18300 Central Avenue, Carson, CA 90746-4008; Toll Free Tel: 800-MAILBOX (800-624-5269); Fax: 800-624-5299; Email: salsbury@mailboxes.com; Web: www.mailboxes.com
B.		Substitutions:  Not permitted.
C.		Requests for substitutions will be considered in accordance with provisions of Section 01600.
2.2 		ALUMINUM MAILBOXES – RACK LADDER SYSTEM
A.			Private Delivery Rear-Loading Aluminum Mailboxes:  Mailboxes with .25 inch (6.35 mm) thick extruded aluminum doors as manufactured by Salsbury Industries consisting of multiple compartments enclosed within recessed wall box. Provide access to compartments for distributing incoming mail from the rear of unit with accessibility to entire group of compartments. Provide access to each compartment for removing mail by swinging compartment door.
1.		Model:  2200 Series Mailboxes – 23.25 inches (591mm) wide by 12.125 inches (308mm) high by 15.5 inches (394mm) deep.
a.		Model 2212:  12 Door Unit - 3.5 inches (89mm) wide by 5.5 inches (139.7mm) high #1 doors.
b.		Model 2208:  8 Door Unit - 5.5 inches (139.7mm) wide by 5.5 inches (139.7mm) high #2 doors.
c.		Model 2204:  4 Door Unit – 10.75 inches (273mm) wide by 5.5 inches (139.7mm) high #3 doors.
d.		Model 2202:  2 Door Unit -  10.75 inches (273mm) wide by 11.5 inches (292.1mm) high #4 doors.
e.		Model 2201:  1 Door Unit – 22 inches (559mm) wide by 11.5 inch (292.1mm) high #5 door.
2.		Model:  2200 Series Parcel Lockers – 23.25 inches (591mm) wide by 12.125 inches (308mm) high by 15.5 inches (394mm) deep.
a.		Model 2270:  1 Door Unit – 22 inches (559mm) wide by 11.5 inches (292.1mm) high door.
b.		Model 2272:  2 Door Unit – 10.75 inches (273mm) wide by 11.5 inches (292.1mm) high doors.
3.		Model:  2200 Series Drop Boxes – 23.25 inches (591mm) wide by 12.125 inches (308mm) high by 15.5 inches (394mm) deep.
a.		Model 2280:  1 Compartment Unit - 23 inches (584mm) wide by 12 inches (305 mm) high door.
b.		Model 2282:  2 Compartment Unit - 11 inches (279mm) wide by 12 inches (305mm) high doors.
4.		Rack Ladders:  .0625 inch (1.6mm) and .25 inch (6.4mm) steel; powder coated finish-black.
a.		Model 2200:  Standard 5 Units High- 15 inches (381mm) wide by 61.875 inches (1,572mm) high by 15.5 inches (394mm) deep.
b.		Model 2200C6:  Custom 6 Units High- 15 inches (381mm) wide by 74.25 inches (1,886mm) high by 15.5 inches (394mm) deep.
c.		Model 2200C4:  Custom 4 Units High- 15 inches (381mm) wide by 49.5 inches (1,257mm) high by 15.5 inches (394mm) deep.
d.		Model 2200C3:  Custom 3 Units High- 15 inches (381mm) wide by 37.125 inches (943mm) high by 15.5 inches (394mm) deep.
e.		Model 2200C2:  Custom 2 Units High- 15 inches (381mm) wide by 24.75 inches (629mm) high by 15.5 inches (394mm) deep.
5.		Mounting:  Recessed mounted.
6.		Locks:
a.	 	Key Lock – Standard: 5-pin cylinder cam lock, 2 keys per lock.
b.	 	Combination Lock – Three digit single dial with spring latch and automatic throw-off.
c.		Spring Latch Lock – 5-pin cylinder cam lock, 2 keys per lock.
d.		Thumb Latch.
7.		Box Identification:
a.		Engraved Placards.
b.		Engraved Doors – Regular.
c.		Engraved Doors – Black-Filled.
d.		Self-adhesive Numbers.
8.		Mail Distribution:
a.		Mail Distribution: Private.
9.		Compartment Material and Finish:  Unfinished surface, 20 gauge.
10.		Door Material and Finish:  Extruded aluminum with powder coated finish.
a.			Color:  Aluminum - standard.
11.		Accessories:
a.		Trim Kit.
b.		Key Blanks.
c.		Rear Locking Cover with Hasp-Full installation height:  20 gauge.
d.		Rear Locking Cover with Standard Lock-Unit height:  20 gauge.
e.		Plexiglass Windows.
PART  3	  EXECUTION
3.1 		EXAMINATION
A.		Verify that openings in wall are correctly located, aligned, and sized for mailboxes.
3.2 		PREPARATION
A.		Clean surfaces thoroughly prior to installation.
3.3 		CLEANING
A.		Clean surfaces with mild dish detergent.  Do not use harsh abrasive cleaners.  Lubricate locks with graphite type lubricants only.
3.4 		INSTALLATION
A.		Install in accordance with manufacturer's instructions.
3.5 		PROTECTION OF INSTALLED PRODUCTS
A.	 	Protect finishes from damage by construction activities.
END OF SECTION