SECTION 10550
(New SECTION 105513, 105523)

MAILBOXES

Display hidden notes to specifier. (Don't know how? Click Here)
PART  1	  GENERAL
1.1 		SECTION INCLUDES
A.		Aluminum Mailboxes - Standard System:  Rear Loading.
1.2 		RELATED SECTIONS
A.		Section 04800 - Masonry Assemblies.
B.		Section 05400 - Cold Formed Metal Framing: Framed wall openings to receive mailboxes.
C.		Section 06100 - Wood Framing: Framed wall openings to receive mailboxes.
D.		Section 09250 - Gypsum Board.
1.3 		REFERENCES
A.		Architectural and Transportation Barriers Compliance Board (ATBCB):  Americans with Disabilities Act Accessibility Guidelines (ADAAG) for Buildings and Facilities.
B.		IBC - International Building Code.
C.		ASTM A 666 - Specification for Austenitic Stainless Steel Sheet, Strip, Plate and Flat Bar.
D.		ASTM B 209 - Specification Aluminum and Aluminum Alloy Sheet and Plate.
E.		ASTM B 221 - Specification Aluminum and Aluminum Alloy Extruded Bar, Rods, Wire, Shapes, and Tubes.
1.4 		SUBMITTALS
A.		Submit under provisions of Section 01300.
B.		[ Product Data ]:  Manufacturer's data sheets on each product to be used, including:
1.		Construction details, material descriptions, dimensions and finishes.
2.		Preparation instructions and recommendations.
3.		Storage and handling requirements and recommendations.
4.		Installation methods.
C.		Shop Drawings:  Prepared specifically for this project; show dimensions of mailboxes, wall cuts, and interface with other products.
1.5 		REGULATORY REQUIREMENTS
A.		Comply with Americans with Disabilities Act Accessibility Guidelines (ADAAG).
1.6 		QUALITY ASSURANCE
A.	 	Manufacturer Qualifications:  Manufacturer shall have a Quality System in place to ensure and be able to substantiate that manufactured units conform to requirements and match the approved design and must be ISO 9001:2015 certified.
1.7 		DELIVERY, STORAGE AND HANDLING
A.		Inspect the materials upon delivery to ensure that specified products have been received.
B.		Store materials protected from exposure to harmful weather conditions.
C.		Handle materials to prevent damage or marring of finish.
1.8 		WARRANTY
A.		Manufacturer's standard warranty to repair or replace components of postal specialties that fail in materials or workmanship within one year from date of Substantial Completion.
PART  2	  PRODUCTS
2.1 		MANUFACTURERS
A.		Acceptable Manufacturer: Salsbury Industries, 18300 Central Avenue, Carson, CA 90746-4008; Toll Free Tel: 800-MAILBOX (800-624-5269); Fax: 800-624-5299; Email: salsbury@mailboxes.com; Web: www.mailboxes.com
B.		Substitutions:  Not permitted.
C.		Requests for substitutions will be considered in accordance with provisions of Section 01600.
2.2 		ALUMINUM MAILBOXES - STANDARD SYSTEM
A.			Private Delivery Rear-Loading Aluminum Mailboxes:  Mailboxes with .25 inch (6.35 mm) thick extruded aluminum doors as manufactured by Salsbury Industries consisting of multiple compartments enclosed within recessed wall box. Provide access to compartments for distributing incoming mail from the rear of unit with accessibility to entire group of compartments. Provide access to each compartment for removing mail by swinging compartment door.
1.		Model:  2200 Series:  23.5 inches (597mm) wide by 30 inches (762mm) high by 15.5 inches (394mm) deep.
a.		Model 2230:  30 Door Unit - 3.5 inches (89mm) wide by 5.5 inches (139.7mm) high #1 doors.
b.		Model 2220:  20 Door Unit - 5.5 inches (139.7mm) wide by 5.5 inches (139.7mm) high #2 doors.
c.		Model 2218:  18 Door Unit – (16) 5.5 inches (139.7mm) wide by 5.5 inches (139.7mm) high #2 doors; (2) 10.75 inches (273mm) wide by 5.5 inches (139.7mm) high #3 doors.
d.		Model 2214:  14 Door Unit -  (12) 5.5 inches (139.7mm) wide by 5.5 inches (139.7mm) high #2 doors and (2) 10.75 inches (273mm) wide by 11.5 inches (292.1mm) high #4 doors.
e.		Model 2210:  10 Door Unit – 5.5 inches (139.7mm) wide by 10.75 inch (273mm) high #2 doors.
f.		Model 2206:  6 Door Unit – (2) 10.75 inches (273mm) wide by 5.5 inch (139.7mm) high #2 doors; (4) 10.75 inches (273mm) wide by 11.5 inches (292.1mm) high #4 doors.
2.		Mounting:  Recessed mounted.
3.		Locks:
a.	 	Key Lock – Standard: 5-pin cylinder cam lock, 2 keys per lock.
b.	 	Combination Lock – Three digit single dial with spring latch and automatic throw-off.
c.		Spring Latch Lock – 5-pin cylinder cam lock, 2 keys per lock.
d.		Thumb Latch.
4.		Box Identification:
a.		Engraved Placards.
b.		Engraved Doors – Regular.
c.		Engraved Doors – Black-Filled.
d.		Self-adhesive Numbers.
5.		Mail Distribution:
a.		Mail Distribution: Private.
6.		Compartment Material and Finish:  Unfinished surface, 20 gauge.
7.		Door Material and Finish:  Extruded aluminum with powder coated finish.
a.			Color:  Aluminum - standard.
8.		Accessories:
a.		Trim Kit.
b.		Key Blanks.
c.		Locking Rear Locking Cover:  20 gauge.
d.		Plexiglass Windows.
PART  3	  EXECUTION
3.1 		EXAMINATION
A.		Verify that openings in wall are correctly located, aligned, and sized for mailboxes.
3.2 		PREPARATION
A.		Clean surfaces thoroughly prior to installation.
3.3 		CLEANING
A.		Clean surfaces with mild dish detergent.  Do not use harsh abrasive cleaners.  Lubricate locks with graphite type lubricants only.
3.4 	INSTALLATION
A.		Install in accordance with manufacturer's instructions.
3.5 		PROTECTION OF INSTALLED PRODUCTS
A.	 	Protect finishes from damage by construction activities.
END OF SECTION